**MG**

 GEKO 14000 RSS CUBE 14KVA

14000 ED-S/SEBA RSS CUBE

 1x 12V DC Socket for DC consumers, powerful synchronous alternator for high starting currents, carrying handles.

1x CEE 32A 3~ socket, 1 CEE 32A 1~ Socket, 2x Schucko (16A)

Optional with IT/TN-power transfer switch for buildings supply

**Mega Genset Malaysia SDN BHD**

[**www.genset**](http://www.genset)**.com.my**

|  |  |
| --- | --- |
| **Alternator** | **Synchronous** |
| El. capacity: 3~ cos φ 0,8 | 13400 VA |
| El. capacity: 1~ cos φ 0,8 | 5900 VA |
| Voltage 3~ | 400 V |
| Voltage 1~ | 230 V |
| Current 3~ | 17,3 A |
| Current 1~ (CEE) | 28 A |
| Current 1~ (Schuko) | 16 A |
| Frequency | 50 Hz |
| Safety class alternator | IP 54 |
| Engine type | B&S 386447 |
| Number of cylinders | 2 |
| Torque-speed | 3000 U min-1 |
| Fuel type | Gasoline |
| Engine oil capacity | 1,7 l |
| Engine power | 13,2 kW |
| Cooling engine/alternator | Air / Air |
| Tank capacity | 19,5 l |
| Operating time: full load / half load | 3,4/6,75 h |
| Weight | 147,5kg |
| Dimensions L x W x H | 820 x 440 x 580 mm |
| Noise power level LWA | 95 dB(A) |



|  |  |  |  |
| --- | --- | --- | --- |
|  **Accessories (optional)**  | **Order No.** |  **Accessories (optional)**  | **Order No.** |
| Exhaust hose  | 904890 | Polarity switch  | 018374 |
| Insulation monitoring  | 018372 | Automatic emergency switch ComAp nano ATS  | 018375 |
| Isolation monitoring with shutdown  | 018369 | Remote start mounting kit 16-pol. with ComAp nano  | 018342 |
| Additional Schuko-socket  | 018370 | Radio remote start/stop with ComAp nano  | 018343 |
| IT/TN-power transfer switch  | 018371 | Operating control ComAp Nano  | 018373 |

Mega Genset Malaysia Sdn Bhd

116 Jalan Tengku Badar,

42000 Port Klang Selangor.

 www.genset.com.my

 Tel: 016-2198537. Fax: 03-31670255,

 www.metallwarenfabrik.com info@metallwarenfabrik.com peter@genset.com.my